Loosen the Four Wing Nuts Holding Chassis Base Cleats Down, Allowing All Possible Clearance Be-
tween Nuts and Base Cleats.

In Transporting In-
strument Wing Nuts Should Be Tightened Down Securely and Again Loosened When Instrument Is In Play-
ing Position.